

*Article*

Pedestrian Safety and the Built Environment: A Review of the Risk Factors

# Philip Stoker1, Andrea Garfinkel-Castro1, Meleckidzedeck Khayesi2, Wilson Odero3,

Martin N. Mwangi4, Margie Peden2, and Reid Ewing1

Journal of Planning Literature 2015, Vol. 30(4) 377-392

ª The Author(s) 2015

Reprints and permission: [sagepub.com/journalsPermissions.nav](http://www.sagepub.com/journalsPermissions.nav) DOI: 10.1177/0885412215595438

[jpl.sagepub.com](http://jpl.sagepub.com/)



Abstract

Urban and regional planning has a contribution to make toward improving pedestrian safety, particularly in view of the fact that about 273,000 pedestrians were killed in road traffic crashes in 2010. The road is a built environments that should enhance safety and security for pedestrians, but this ideal is not always the case. This article presents an overview of the evidence on the risks that pedestrians face in the built environment. This article shows that design of the roadway and development of different land uses can either increase or reduce pedestrian road traffic injury. Planners need to design or modify the built environment to minimize risk for pedestrians.

Keywords

pedestrian safety, risk factors, built environment

# Introduction

Road traffic injuries are the eighth leading cause of death glob- ally, and the leading cause of death for young people aged fif- teen to twenty-nine (World Health Organization 2013a). Current trends suggest that by 2030 road traffic deaths will become the fifth leading cause of death unless urgent action is taken (Peden et al. 2004; World Health Organization 2013a). In particular, nations such as India, China, and other countries with burgeoning populations and rapidly growing motorization and urbanization face a substantial increase in pedestrian injuries and fatalities (Zegeer and Bushell 2012). Now that over half of the global population lives in cities, the same concern for pedestrian safety is likely wherever urbani- zation and motorization are causing more people to be on the roads.

Of the over one million road traffic deaths annually, nearly one-quarter (22 percent) are pedestrians, 5 percent are cyclists, 23 percent are motorcyclists, 31 percent are car occupants, and 19 percent are other groups or unspecified (World Health Orga- nization 2013a). Another fifty million people worldwide are injured as a result of traffic collisions (World Health Organiza- tion 2013a). Several of the established causes of these fatalities and injuries are related to the built environment: traffic volumes, excessive roadway speed, poor lighting, and urban development patterns. As planners, we need to recognize what risks to pedes- trians result from the design of the built environment.

Many of the solutions to reducing these risk factors are within the range of influence and control of planners. However, to effectively address and mitigate risks to pedestrians, plan- ners need to understand the risk factors that affect pedestrian

safety. We examine the built environment as a factor that raises or minimizes the probability of pedestrian injury and death, in line with the definition of risk offered in the World Health Report of 2002 (World Health Organization 2002). This litera- ture review synthesizes some of the most recent research on pedestrian safety and the built environment from around the world. This article begins by briefly describing the types of pedestrians. We then present a conceptual model of the rela- tionship between the built environment and the pedestrian safety and present evidence of the risk factors pedestrians face in the built environment. We highlight the connections between the risk factors. This review can serve as a resource for planners to understand the risk factors, and how the risk factors interact, in order to guide safety-oriented policies and design.

## *Method and Approach*

We conducted the literature review on key databases (e.g., SCOPUS, Web of Science, PubMed, and Google Scholar) using the following key words to find relevant literature:

1 City and Metropolitan Planning, University of Utah, Salt Lake City, UT, USA 2 Department of Violence and Injury Prevention, World Health Organization, Geneva, Switzerland

3 School of Public Health, Maseno University, Kisumu, Kenya

4 Wageningen University, Wageningen, the Netherlands

Corresponding Author:

Philip Stoker, City and Metropolitan Planning, University of Utah, 375 S. 1530 E. #235 AAC, Salt Lake City, UT 84108, USA.

Email: [philip.a.stoker@gmail.com](mailto:philip.a.stoker@gmail.com)

Table 1. Pedestrian Categories.

Pedestrian Type Description

Relative Risk

Factor Source

Young children Approximately 21 percent of road traffic deaths

involve young children

Young adults For fifteen- to twenty-one-year-olds, pedestrian

fatalities are the leading cause of death

Male pedestrians Males are overrepresented in pedestrian fatalities in most but not all studies

Gender roles Women and girls in low-income countries walk more

and transport more household goods than male counterparts, increasing their risk as pedestrians

Elderly The elderly have the highest risk of mortality of all pedestrians when involved in vehicle collisions

Very high Barton and Schwebel (2007), Peden

(2004), and Peden et al. (2008) Above average Hilton (2006)

Above average Goren et al. (2005), Durak et al. (2008),

and Tom and Granie´ (2011)

Above average Rosenbloom and Plessis-Fraissard

(2009) and Roy (2009)

Very high Assailly (1997), Davies et al. (1999),

Vyrostek, Annest, and Ryan (2004), Retting et al. (2003), Gawryszewski and Rodrigues (2006), and Ponnaluri and Nagar (2010)

Low socioeconomic status

Intoxicated or distracted pedestrians

A strong inverse relationship is found between socioeconomic status and risk of pedestrian injuries and fatalities

Intoxication and distraction from mobile devices put pedestrians at higher risk for pedestrian injuries and fatalities

High Marcin et al. (2003), Cubbin (2002), and Azetsop (2010)

High Clayton and Colgan (2001), Stavrinos, Byington, and Schwebel (2009), Nasar, Hecht, and Wener (2008), and Hatfield and Murphy (2007)

Disabled pedestrians Visually impaired pedestrians are elevated at risk

from drivers who yield inconsistently and unreliably; disabled youths are especially vulnerable pedestrians

High Guth et al. 2005 and Xiang et al. 2006

Pedestrians in low- income countries

Pedestrians in low-income countries are particularly vulnerable to injury and death from collisions, attributable to increasing urbanization, and motorization inadequate pedestrian facilities, lack of pedestrian safety education, and access to emergency health care

Above average Peden and Hyder (2002), Peden et al.

(2004), and Bishair et al. (2006)

pedestrian safety, pedestrian accidents, pedestrian injuries, pedestrian fatalities, pedestrian crashes, pedestrian education, pedestrian education in developing countries, and so on. We focused primarily on the most recent research available.

The initial review of research articles and their bibliographies provided a wealth of follow-up citations. Tracing backward, we compiled and reviewed both published and unpublished reports, as well as published academic articles. The literature on pedes- trian safety and the relationship between the pedestrian safety and the built environment is vast and our modest effort in this article is to provide an overview of the evidence that may be used for decisions by planners. Apart from the literature on pedestrian safety, there is the issue of the most appropriate way to organize a literature review that cuts across countries at differ- ent levels of development as well as varying conditions in the built environment. We explored different options, including focusing on different development contexts or selected themes as the basis to present the literature. We opted to use selected themes in an effort to show some variation in pedestrian road traffic injuries by contextual factors such as countries and rural/urban sites. It is a modest effort at comparative analysis and we hope readers will isolate the key risk factors presented through a mix of contexts from around the world. We believe

planners need to appreciate the mix of environments in which pedestrian crashes occur.

# Types of Pedestrians

Pedestrians form a mixed group of people with respect to age, gender, travel behavior, and socioeconomic status (SES). This body of research and literature focuses specifically on pedes- trians, how they can be categorized, and their relative risk fac- tors. While certain categories of pedestrians are specific to locale (such as low socioeconomic pedestrians or gender- related roles in low-income countries), and although research is typically carried out within regional or national geographies, much research is generalizable to a pedestrian type. Table 1 presents broad categories of pedestrian types, described in detail subsequently, that are at elevated risk for pedestrian- related injuries and fatalities. A general ranking of relative risk is assigned, based on the literature: severity of risk identified by research and the volume of confirmatory research and lit- erature. Sources identified in Table 1 represent major works, and further additional literature is found by types mentioned subsequently.

## *Young Children and Young Adults*

Children are particularly at risk in road traffic crashes (Assailly 1997; Davies et al. 1999; Vyrostek, Annest, and Ryan 2004; Retting et al. 2003; Gawryszewski and Rodrigues 2006; World Health Organization 2009; Ponnaluri and Nagar 2010). Approximately 21 percent of road traffic fatalities are children, resulting in an average of 720 child deaths related to road traffic crashes daily (Peden et al. 2008). Traffic injuries are the second leading cause of death worldwide for young children (Peden 2004) and are the leading cause of childhood disability worldwide (Peden et al. 2008).

Some explanations of why children are at particular risk include their underdeveloped abilities and perceptions (Constant and Lagarde 2010) and greater variability in their actions (Pitcairn and Edlmann 2000). Many children begin to experience mobility and independence at a young age but are not yet cognitively capable of safely navigating traffic condi- tions (Barton and Schwebel 2007). Compounding this risk is their small size, which makes them both less visible to drivers and more vulnerable to injury and death in collisions (Barton and Schwebel 2007).

Some studies have shown that as a parent’s level of education increases, the risk of child pedestrian injury decreases (Agran et al. 1998; Pless, Verreault, and Tenina 1989; Rivara and Barber 1985). However, it is not parental education alone that influ- ences risk. In an experiment testing the effects of parental super- vision, Barton and Schwebel (2007) found that parental supervision in pedestrian crossings moderated the risky behavior children exhibited. Interestingly, though, if parents display risky behavior, the children will do the same. In a survey on child–par- ent interaction, mothers were much more likely than other fam- ily members to provide some form of road safety education and set a good example as safe road users while pointing out unsafe behaviors by others (Green et al. 2008).

The school–home journey is a point of considerable expo- sure and risk for children. Roberts (1995) found strong evi- dence that children accompanied by an adult during the school–home journey significantly reduce their risk of injury or death. The Walking School Bus and Safe Routes to School are two of a number of school- and community-based pro- grams designed to increase children’s safety during the walk- ing journey to and from school (Heelan et al. 2009; Mendoza, Levinger, and Johnston 2009), and while these are generally successful (Boarnet et al. 2005), they have some critics (Collins and Kearns 2005; Kearns, Collins, and Neuwelt 2003). These critics stress that the predominance of motorized travel and design standards to accommodate and prioritize travel by cars outweighs the benefits derived from safe travel programs to and from school. Until design standards are changed, these programs are unlikely to really address the heart of the problem.

## *Male Pedestrians*

Many studies find that male pedestrians of all ages are over- represented in pedestrian collisions. Almost two-thirds of

children killed as pedestrians are male, and they have a death rate of 57 percent higher than of female children (Goren et al. 2005; Durak et al. 2008; Tom and Granie´ 2011). Some researchers suggest that males are more likely than females to violate pedestrian rules (Tom and Granie´ 2011). However, other studies find no relationship between a pedestrian’s sex and their risk for injury or mortality (Moe 2008; Ibrahim et al. 2012; Dandona et al. 2008). We report findings that have found that male pedestrians are overrepresented in pedestrian collisions. One explanation is a willingness to engage in risky behaviors. However, we follow this section with the ‘‘Gender roles’’ subsection and report findings that in certain situations, women are at greater risk as pedestrians than males.

## *Gender Roles*

In low-income countries, gender-based roles factor enormously in the time men versus women spend as pedestrians. Walking, as a form of transport, falls on girls and women far more than boys and men (Rosenbloom and Plessis-Fraissard 2009). In the forty-five poorest countries in the world, where one-fifth of the world’s population lives, women walk more and far more often carry heavy loads of household goods that include children, water, and wood (Rosenbloom and Plessis-Fraissard 2009; Roy 2009); this is particularly so in sub-Saharan Africa. In addition to hazards resulting from roads that are poorly designed, devel- oped, and maintained (Rosenbloom and Plessis-Fraissard 2009), women in developing countries are highly vulnerable pedestrians due to cultural conditions that leave them subject to ‘‘sexual harassment, crime, violence .. . pollution and noise’’ (Seedat, MacKenzie, and Mohad 2006, 150).

Despite the load-carrying burdens placed on women in many parts of the world, minimal research has been conducted to date to identify precisely the added risk factors to women under these circumstances. Extrapolating from the literature on the impacts of backpack loads to mobility (see Wang, Pas- coe, and Weimar 2001; LaFiandra et al. 2003; Chow et al. 2005; Negrini and Carabalona 2002), it is conceivable that women with portage (loads) are at measurably higher risk for vehicle–pedestrian crashes than are men. The noted lack of research on gendered pedestrian issues in low-income countries continues to leave many questions unanswered (Porter 2002, 2008; Rosenbloom and Plessis-Fraissard 2009).

## *Elderly Pedestrians*

The number of older persons (those who are sixty years and over) is growing steadily in the world. In 2013, there were 841 million older persons in the world (United Nations 2013). This number is expected to more than double, to more than two billion in 2050. It is also projected that older persons are to exceed the number of children for the first time in 2047 (United Nations 2013). There is global variation in the distribu- tion of the population of older persons, with about two-thirds of the world’s older persons living in developing countries. It is estimated that by 2050, nearly eight in ten of the world’s older

population will live in the world’s less developed regions (United Nations 2013). There is also variation in the older pop- ulation. Analysis shows that the population aged eighty years or over is occurring at a faster pace in the less developed regions than in the more developed regions (United Nations 2013). The aging population has implications for transport planning, especially in ensuring safe accessibility of older per- sons to services and facilities as they fulfil their roles in society. Walking is the primary mode of transportation for the elderly worldwide (Siram et al. 2011) and an important source of independence for the elderly (Langlois et al. 1997), provid- ing important health benefits, as well (Kerr, Rosenberg, and Frank 2012). As pointed out by Whitelegg (1993), older people need special consideration in the design of the built environ- ment and road traffic environment in which they live and where they access local shops and services such as trips to the doctor, dentist, optician, and other services used intensively by this age-group. Studies on aging and transport also indicate that pedestrian safety is an important safety concern for the elderly (Peden et al. 2004; Whitelegg 2012). Several factors work together to increase the risk of older pedestrians (World Health

Organization 2013b):

Deterioration in visual acuity may have a negative impact on their ability to cross the road safely. In gen- eral, older pedestrians look less at traffic and accept sig- nificantly smaller gaps in traffic when crossing the road than younger pedestrians.

•

Reduced mobility can render older pedestrians unable to react quickly in imminent danger to avoid a crash.

•

Underlying health conditions or frailty can result in greater injury severity when a crash occurs.

•

Reduced speed when crossing the road: the speed of elderly pedestrians does not itself increase risk; rather, the risk comes from the speed of the traffic and, in par- ticular, from automated signals that do not allow suffi- cient time for slower pedestrians to cross safely and completely. In many municipalities, the assumed walk- ing speed used to set crossing times at signalized cross- ings is faster than an older person can walk, leaving them stranded on the road when the signal phase changes to allow vehicle movement (Job et al. 1998). Whitelegg (1993) points out that transport planning and practice based on encouraging motorization and car-based trips achieves its success by stealing time from other groups especially elderly pedestrians who must now spend more time waiting to cross a road or be diverted through an unpleasant underpass; having to negotiate ugly metal bar- riers that obstruct direct walking routes; or find that local services they prefer to use have closed and they must now travel longer distances to shopping centers, hospitals, or clinic because they have relocated to more inaccessible, pedestrian-unfriendly locations.

•

The combined effects of the above-mentioned risks are revealed in research, showing that the elderly suffer the highest

mortality rates in pedestrian crashes (Small and Sheedy 2006; Bhalla et al. 2009; Zhao et al. 2010; Bartels et al. 2010). Studies unanimously find that the severity of injury from a traffic colli- sion is related to the resilience of the pedestrian (Methorst et al. 2010), with elderly pedestrians likely to experience more trauma than other adult pedestrians (Demetriades et al. 2004).

## *Low SES Pedestrians*

SES is a mediating factor of pedestrian risk and injury (Sharples et al. 1990; Marcin et al. 2003; Cubbin 2002; Azetsop 2010), with a strong inverse association to fatal injuries (Cubbin 2002). A majority of child pedestrian injuries are asso- ciated with low income and poverty status (Rivara and Barber 1985). In the United States, children from families earning less than US$20,000/year are seven times more likely to be injured than children from families earning more than US$30,000/year (Mueller, Rivara, and Bergman 1988). Chakravarthy et al. (2010) found that the percentage of the population living in low-income households is the strongest predictor of pedestrian injuries, with pedestrian crashes four times more likely in poor neighborhoods. This finding is repeated in a study that found that the risk of injury for children in the lowest socioeconomic stratum is more than twice that of children in higher SES cate- gories (Roberts et al. 1995). A further study found that the risk of injury for children in the lowest socioeconomic stratum is more than twice that of children in higher SES categories (Roberts et al. 1995). A study of Buffalo, New York, found bicycle and pedestrian crashes were related to some SES factors (ethnicity and educational status) but not all factors (income), and land use played a factor in crashes, while infrastructure impacts were minimal (Delmelle, Thill, and Ha 2012).

While factors related to poverty, such as age, education, lan- guage fluency, and population density do not explain the effects of poverty on pedestrian injuries, exposure explains some of the increased risk. A survey of Indian children in Hyderabad reported that as household income increased, the proportion of pedestrian trips decreased and trips by bicycle or motorized two-wheeled vehicles increased, significantly reducing the likelihood of pedestrian injury for children in the highest household income quartile (Dandona et al. 2008). A similar pattern is observed internationally, where higher income countries record lower levels of pedestrian activity and lower levels of pedestrian fatalities, whereas lower- and middle-income countries experience higher levels of both (World Health Organization 2009).

## *Intoxicated or Distracted Pedestrians*

As temporary conditions, these two statuses are combined into a single type of pedestrian, representing high though temporal risk. Research suggests that intoxicated pedestrians are at sig- nificantly higher risk of injury (Clayton and Colgan 2001). In a review of Australian studies, Holubowycz (1995) determined that 20–30 percent of pedestrians involved in collisions had

blood alcohol content (BAC) levels in excess of 0.15 g/dl, with higher BAC levels more frequently resulting in fatalities. Peden et al. (2004) found that in South Africa, alcohol was a factor in over 61 percent of fatal pedestrian collisions. A recent study in the United Kingdom concluded that nearly half of all pedestrians killed in road traffic collisions had been drinking (Keigan and Tunbridge 2003).

Mobile electronic devices appear overall to present an increased risk to pedestrian safety (Hatfield and Murphy 2007; Nasar, Hecht, and Wener 2008; Neider et al. 2010; Stavrinos, Byington, and Schwebel 2009). Talking on a mobile phone is shown to reduce situational awareness, creating poten- tially treacherous environments for pedestrians. A study by Nasar, Hecht, and Wener (2008) found that mobile phone users engaging in conversation were significantly more likely to make unsafe road crossing decisions compared to subjects not using mobile devices. The evidence on the safety effects of per- sonal music devices is less clear than it is for mobile phones. One study using a virtual environment found subjects operating a hands-free mobile phone were more likely to make dangerous road crossing decision than those using electronic music devices (Neider et al. 2010). Another similar study found that subjects using either a mobile phone or a music device were at increased risk of being hit in a virtual environment (Schwe- bel et al. 2012). Walker et al. (2012) found little difference in cautionary behavior between pedestrians using versus not using mobile music devices. Finally, Hatfield and Murphy (2007), Nasar, Hecht, and Wener (2008), and Stavrinos, Byington, and Schwebel (2009) all conclude that the use of cell phones, earphones, and other electronic devices are distractions that increase the risk of injury or death for pedestrians.

## *Disabled Pedestrians*

Pedestrians with physical disabilities do not comprise a high number of pedestrians overall, yet are at particularly high risk for injury or death. Visually impaired pedestrians were found to have greater difficulty navigating higher volume, multiple-lane roundabouts compared to single lane roundabouts (Guth et al. 2005). They also found that drivers were unreliable and incon- sistent in their willingness to yield to blind pedestrians, even when using canes or guide dogs (Guth et al. 2005). Research on disabled pedestrians aged five to seventeen found they were five times more likely to be involved in a collision compared to those without a disability (Xiang et al. 2006).

## *Pedestrians in Low-income Countries*

Nearly all countries with the highest absolute numbers and rates of pedestrian fatalities are developing countries (Toroyan 2009). Approximately 96 percent of children killed worldwide due to road traffic injuries live in low- and middle-income coun- tries (Peden et al. 2004). Pedestrians account for 42 percent of all road traffic deaths in Delhi, India, and 38 percent in Colombo, Sri Lanka (Bishair et al. 2006). The continuing levels of growth of urbanization/suburbanization and motorization now occurring




Figure 1. Conceptual framework linking the built environment to pedestrian safety.

in developing nations, pedestrian injuries, and deaths potentially jeopardize the pursuit of health equity (Peden and Hyder 2002; Bishair et al. 2006; Wilkinson and Marmot 2003). Low- income countries are particularly challenged to allocate funding for pedestrian facilities and services (Zegeer and Bushell 2012), making road crossing especially dangerous due to poor lighting, heavy- and high-speed traffic, limited traffic law enforcement, lack of safety education, and poor access to emergency health facilities (Berger and Mohan 1996; Nakitto et al. 2008).

# The Built Environment and Pedestrian Safety

The physical context of pedestrian safety is the built environ- ment, the focus of this part of the article. The conceptual frame- work relating the built environment to pedestrian risk is presented in Figure 1. The framework is organized by scale, from regional scale at the top of the figure to street scale at the bottom of the figure. We account for interactions between the spatial and administrative scales: development patterns of the built environment at the regional scale, such as density, urban sprawl, and regional development all produce character- istics of the built environment at the local scale: pedestrian infrastructure and roadway design. For example, in a rural region, there is likely to be little pedestrian infrastructure and roadway designs typically facilitate auto travel but do not accommodate pedestrians. Conversely, in highly dense urban settings, there may be more facilities for pedestrians and the roadway design may be more accommodating to pedestrians. In either case, the characteristics of the built environment at the local scale produce traffic and pedestrian conditions related to

pedestrian safety: visibility, traffic volumes, and traffic speed. The visibility of pedestrians may increase or decrease depend- ing on pedestrian infrastructure such as crossing lights. Or there may be characteristics of roadway and urban design that increase visibility such as elevated crossings and street lights. Traffic volumes and traffic speed are affected primarily by roadway and urban design, where traffic conditions at the street scale are a result of the design of the built environment at local scale.

Each of these three conditions has an effect on the risk of collision, injury, and death for pedestrians. Lower visibility for pedestrians increases this risk of a collision, higher traffic volumes increase crash frequency, and higher traffic speed increases the severity of the crash. The overall risk to a pedes- trian is the combination of the risk from the built environment plus the risk relative to the type of pedestrian. The literature related to each of the components of the conceptual framework is synthesized subsequently.

## *Development Patterns: Density*

Vehicular and pedestrian traffic tend to increase with develop- ment density, as do vehicle–pedestrian collisions. In a Califor- nia study, Agran et al. (1996) found that the incidence of injury for children living in high-density residential areas was three times higher than that of children living in single-family resi- dences. Similarly, LaScala, Johnson, and Gruenewald (2001) found that pedestrian injuries occurred more often in areas with higher populations and greater cross-street densities. The den- sity of development affects characteristics of the built environ- ment such as roadway design and pedestrian infrastructure. For example, Clifton and Kreamer-Fults (2007) found that transit access, commercial land uses, and high population densities had direct relationships to pedestrian crashes near public schools. These researchers also found that characteristics of the built environment such as roadway design (e.g., the access to driveways) had a significant negative impact on pedestrian safety. Each of these characteristics is related to the density of development at a regional scale.

While there is little doubt that the absolute number of pedes- trian crashes increases with development density, the relation- ship between the two appears not be linear. Collision rates relative to exposure may actually decline with rising densities, and the severity of injuries certainly declines. In a study enti- tled ‘‘Safety in Numbers: More Walkers and Bicyclists, Safer Walking and Bicycling,’’ Jacobsen (2003, 205) tapped several data sources to show that crashes between motorists and pedes- trians or cyclists were less likely when people walking or bicy- cling in the immediate area increased. In an environment with many pedestrians or bicyclists, motorists may be more aware of them and adjust their driving behaviors accordingly. Although plausible, some have criticized the ‘‘safety in numbers’’ theory as simplistic and have argued to focus on local-level character- istics of the built environment: roadway design, speed policies, and increased investment on pedestrian infrastructure (Bhatia and Wier 2011).

Studies that seek to infer causal relationships between den- sity and pedestrian collisions must contend with multiple con- founding variables: more residents, more employment, more roads, and more of everything (Ewing and Dumbaugh 2009). As a result, density alone may not be a predictor of the risk in the built environment. Rather, the relationship between pedestrian risk and development density is linked through vehi- cle miles traveled (VMT). As VMT increases, traffic collisions (of which pedestrians injuries are a substantial part) increase (Ewing and Dumbaugh 2009). Therefore, pedestrian risk is related to the overall VMT generated by the density of devel- opment. Research from North America indicates that as devel- opment density increases, VMT decreases (Ewing and Cervero 2001). Therefore, the contradiction found in the literature regarding density and pedestrian collisions is clarified by understanding the relationship between density and VMT.

## *Development Patterns: Regional Development*

The rate and severity of crashes tend to be highest wherever the bulk of the population resides. For example, in the United Kingdom, young pedestrians from urban areas were involved in collisions five times more frequently than those in rural areas, and their death rate was twice as high (Petch and Henson 2000). Similarly, Odero, Khayesi, and Heda (2003) found that pedestrians were more likely to be killed in urban areas. Pedes- trian fatality and injury rates may differ between urban and rural regions because pedestrian volumes and vehicle operating speeds differ. Consequently, if a region’s population is predo- minantly rural, this is where most of the collisions will occur. Conversely, if a country’s population is predominantly urban, most of the collisions will occur in urban areas.

Beyond these facts, the evidence suggests that pedestrians in rural places have higher rates of injuries and their injuries tend to be more severe than pedestrians in urban areas (Mueller, Rivara, and Bergman 1988; Litman and Fitzroy 2005; Ewing and Dumbaugh 2009; Ibrahim and Sayed 2011; Tarko and Azam 2011). For example, in Ghana, residents are 58 percent more likely to die in traffic collisions on rural than on urban roads (Afukaar, Antwi, and Ofosu-Amaah 2003) and in Kenya, a majority of road traffic injuries occur on rural roads (Odero, Garner, and Zwi 1997). In Pakistan, twice as many road deaths occur in rural areas as in urban areas (Shah, Khoumbati, and Soomro 2007). Ma et al. (2010) found that in China, pedes- trians commuting in rural contexts were more likely to be injured in a traffic collision than those commuting within urban areas. This is consistent with earlier studies showing generally higher pedestrian injuries in rural areas (Al-Madani and Al-Janahi 2006; Xie et al. 2002).

There are several explanations for why rural areas appear to be more dangerous for pedestrians. One is that the relationship between VMT and traffic fatality rates is roughly linear. VMT per capita are consistently higher in rural areas, with corre- spondingly higher fatality rates per capita (Litman and Fitzroy 2005; Ewing and Dumbaugh 2009). Rural roads also produce characteristics of the built environment that promote higher

traffic speeds than urban roads. Measures to reduce traffic speeds in rural China resulted in improved pedestrian safety (Changcheng et al. 2010). Additionally, pedestrian crashes in rural areas are generally located farther from emergency medical facilities, and emergency services take longer to arrive at the scene of a crash to provide lifesaving medical care (Mueller et al. 1988). Rural roads are also less likely to include complete characteristics of the built environment such as pedestrian infrastructure. Wanvik (2009), for example, found that while pedestrian risk for injury on rural Dutch roads increased 140 percent during nighttime hours on roads with lighting, whereas the risk increased by 360 percent on rural roads without lighting.

## *Development Patterns: Urban Sprawl*

For the same reasons, pedestrian crashes are more likely to be fatal in rural areas, pedestrian–vehicle crashes are more likely to be fatal in sprawling urban areas. Urban sprawl, prevalent internationally and particularly common in North America, is characterized by four dominant qualities: a widely dispersed population and low-density development; the rigid separation of residential, commercial, industrial, and office uses; poorly defined activity centers; and a road network typified by large blocks and poor connectivity (Ewing, Pendall, and Chen 2002). In an extensive study, Ewing, Schweiber, and Zegeer (2003) found associations between the degree of sprawl and traffic fatalities, with each 1 percent decrease in sprawl result- ing in 1.49 percent decrease in traffic-related fatalities overall, and between 1.47 and 3.56 percent decrease specifically in pedestrian fatality rates.

Relatively high numbers of miles of arterial roadways and the presence of strip malls and big-box stores (indicative of urban sprawl) are also determinants of traffic injury rates (Dumbaugh and Li 2011). A substantial study by Marshall and Garrick (2011) analyzed 230,000 crashes occurring over eleven years in California, finding that denser street networks with higher intersection counts—the converse of urban sprawl—was associated with fewer crashes across all severity levels. Like- wise, vehicle–pedestrian collisions occurring at intersections in neighborhoods with mixed land uses and nearby schools— also the converse of urban sprawl—resulted in lower rates of injury and death compared to collisions in other development types (Zahabi et al. 2011). Again, the link between pedestrian safety and development patterns is VMT.

## *Characteristics: Pedestrian Infrastructure*

Pedestrian infrastructure can reduce pedestrian exposure to vehicular traffic and reduce vehicle speeds (Lonero, Clinton, Sleet 2006; Zeeger et al. 2004; Retting, Ferguson, and McCartt 2003; Peden et al. 2004; Elvik et al. 2009; Sleet, Naumann, and Rudd 2011; Zegeer and Bushell 2012; World Health Organiza- tion 2013b). These street treatments are briefly summarized subsequently and organized by reducing pedestrian exposure and reducing vehicle speeds.

## *Street Treatment: Reducing Pedestrian Exposure to* Vehicular Traffic

The specific engineering measures that reduce pedestrian expo- sure to vehicular traffic by either creating separation between pedestrians and vehicles or reducing traffic volume are side- walks and footpaths, marked crossings, overpasses and under- passes, and mass transport routes.

## *Street Treatment: Reducing Vehicle Speeds*

As pointed out in several studies and reports (e.g., World Health Organization 2013b), speed is a key risk factor for pedestrian traffic injury. Hence, speed management remains an effective measure to reduce pedestrian traffic risk. The engi- neering approach to speed management consists of a number of specific traffic-calming measures: physical treatments to roads as well as perceptual treatments and speed limit reductions aimed at reducing vehicle speeds and sometimes traffic volume (Mead et al. 2014). Traffic-calming measures are generally of two types: (a) those that require motorists to change their direc- tion of travel by moving either to the left or right and (b) those that require motorists to change elevation by either going up or down (Vanderschuren and Jobanputra 2009). Traffic-calming measures can vary from a few minor changes, through modifi- cations of local streets, to area-wide changes and major rebuilds (Vanderschuren and Jobanputra 2009). Their effects include moderate speed reductions to street design changes, with various degrees of success in reducing pedestrian crashes and traffic volume (Table 2). A number of studies show a reduction in pedestrian–vehicle conflicts and crashes associ- ated with refuge islands, marked crossings with raised medians, road narrowing, staggered lanes, road humps, and junction redesign (World Health Organization 2013b).

## *Characteristics: Roadway Design*

In general, streets designed to be narrower and for slower speeds experience the lowest rates of vehicle–pedestrian crashes, while wide street lanes and higher operating speeds experience the highest rates (Garder 2004). For these reasons, European road- way engineers design for lower vehicle operating speeds in developed areas (Federal Highway Administration 2001; Lamm, Psarianos, and Mailender 1999; Organisation for Economic Co-operation and Development 1998; UK Department for Transport 2007). In the Netherlands, a ‘‘sustainable safety’’ policy sets roadway speed limits based on road function with this policy potentially resulting in one-third fewer injuries per million vehicle kilometers (Institute for Road Safety Research 1993).

Conversely, roadway expansion and widenings occur at the expense of safety, even after controlling for traffic volumes (Dumbaugh 2005; Harwood 1986; Milton and Mannering 1998; Noland and Oh 2004; Sawalha and Sayed 2001; Vitaliano and Held 1991; Hummer and Lewis 2000). Wide lanes adversely affect traffic safety, particularly in urban areas.

Table 2. Traffic-calming Measures, Their Application, and Impact.

Speed Reduction Can Be Applied to

|  |  |  |  |
| --- | --- | --- | --- |
| Type | Arterial Roads | Local Roads | Impact  on Traffic Volume |
| Speed hump | No | Yes | Possible |
| Speed table | With caution | Yes | Possible |
| Raised crosswalk | Yes | Yes | Possible |
| Raised intersection | With caution | Yes | Possible |
| Textured pavements | Yes | Yes | Possible |
| Speed cushion | With caution | Yes | Possible |
| Rumble strips | Yes | Yes | No |
| Traffic (mini) circle | No | Yes | Possible |
| Roundabout | Yes | Yes | Not likely |
| Chicanes | No | Yes | Yes |
| Realigned intersection | Yes | Yes | Possible |
| Tight radii | Yes | Yes | Possible |
| Centre island narrowing | Yes | Yes | Possible |
| Chokers | Yes | Yes | Possible |
| Road diets (i.e., lane reduction) | Yes | Yes | Yes |
| Speed limits | Yes | Yes | No |
| Speed alerts, enforcement | Yes | Yes | No |
| Perceptual design | Yes | Yes | Possible |
| Warning signs | Yes | Yes | No |
| Half closure | Yes | Yes | Yes |
| Diagonal diverters | Yes | Yes | Yes |
| Lateral shift | Yes | Yes | No |
| Median barriers | Yes | No | Yes |
| Gateway treatments | Yes | No | No |
| Traffic signal coordination | Yes | No | No |
| Vehicle-activated signs | Yes | No | No |

*Source:* Vanderschuren and Jobanputra (2009).

Noland and Oh (2004) found that wider lanes were associated with statistically significant increases in total and fatal crashes in the state of Illinois. Lee and Mannering (1999) established that while wide lanes reduced the probability of run-off- roadway crashes in rural settings, they were associated with increases in these types of crashes in urban areas. In reexamin- ing the historical literature on lane widths and traffic safety, Hauer (1999) found that research from 1940 forward consis- tently showed crashes increasing as lanes exceed eleven feet in width. These results are confirmed by Swift, Painter, and Goldstein (2006) who found that after examining thirteen phy- sically built environment characteristics for approximately 20,000 collisions report street width correlated most highly with collision rates, and the safest streets are found to be nar- row (twenty-four foot wide) and slow.

Traffic speed, discussed subsequently as impacting injury severity in collisions, can be reduced by narrowing lanes and shortening street sections (Harwood 1990; Farouki and Nixon 1976; Heimbach, Cribbins, and Chang 1983; Clark 1985; Gattis and Watts 1999; Gattis 2000; Fitzpatrick et al. 2001). Drivers on narrow streets generally behave less aggressively, run fewer traffic signals, and drive slower (Untermann 1990). This may be because drivers feel less safe and therefore drive more cautiously on narrow streets (Ewing and Dumbaugh

2009). Studies of ‘‘road diet’’ projects, which reduce the num- ber of traffic lanes on a road, find that traffic crashes decrease as lanes are eliminated (Huang, Stewart, and Zegeer 2002; Knaap and Giese 2001). One possible explanation is that on two-lane roads, prudent drivers set the pace and others must follow, whereas on multilane roads where passing is possible, high-speed drivers set the prevailing speed (Burden and Lager- wey 1999).

One of the strategies developed in the Netherlands for traffic calming is known as woonerf, a residential area (sometimes referred to as a ‘‘living yard’’) that promotes sharing of the street by pedestrians, cyclists, and motorists but giving priority to pedestrians and cyclists. Vehicles are allowed on the streets under the strict conditions of low speed, nonobtrusive parking, and limited traffic (Woonerfgoed Network 2014). The woonerf basically seeks to strike a balance between the life of a commu- nity and the movement of vehicles. The woonerf has spread from the Netherlands where it started in the 1970s to other parts of the world. The concern about livable streets and rebalancing the needs of different road users is spreading around the world (Khayesi, Monheim, and Nebe 2010). There are several pro- gram initiatives and policy efforts toward this end such as home zone, complete streets, residential zone, shared zone, shared space, and walkable communities.

## *Conditions: Traffic Volumes*

Research worldwide consistently finds that the higher the traf- fic volume, the greater the frequency of pedestrian injuries (Quaye et al. 1993; Roberts et al. 1995; Agran et al. 1996; McMahon et al. 2002; Hijar, Vasquez-Vela, and Arreola-Risa 2003; Harwood et al. 2008; Chen, Meng, and Wang 2009; Ma et al. 2010). In one study, Roberts et al. (1995) found that the risk of injury for children was thirteen times higher in neighborhoods with the highest traffic volumes compared to those with the lowest. In another, Quaye et al. (1993) found that the probability of a pedestrian injury with a left-turning vehicle varied as a function of traffic volume. And Harwood et al. (2008) demonstrated that higher traffic volumes at signalized intersections were associated with a higher likelihood of pedes- trian crashes. Data from crash records in China between 2004 and 2007 result in the finding that arterial roads with heavier traffic volumes tended to have more severe crashes (Ma et al. 2010). Finally, specific peak periods of pedestrian and vehicle traffic volume, such as holidays, are associated with higher lev- els pedestrian injuries and fatalities (Road Traffic Management Corporation 2009).

## *Conditions: Traffic Speeds*

The risk factor that increases the severity of pedestrian injuries and fatalities is traffic speed (Mohan and Tiwaria 1998; Hijar, Vasquez-Vela, and Arreola-Risa 2003; European Transport Safety Council [ETSC] 1999). Vehicle speeds are repeatedly associated with increased injury severity and death in motor vehicle collisions involving pedestrians (Anderson et al. 1997;

Avineri, Shinar, and Susilo 2012; ETSC 1999; Garder 2004; Grundy et al. 2009; Hijar, Vasquez-Vela, and Arreola-Risa 2003; Kim et al. 2010; Mohan and Tiwaria 1998; UK Depart- ment of Transport 1997; Zegeer et al. 2002; Zhao et al. 2010; Zegeer and Bushell 2012). Simple physics tells us that higher vehicle-operating speeds give drivers less time to react to unfore- seen hazards, cause drivers to travel farther before stopping when hazards are present, and result in increased force of impact when crashes occur.

Evidence indicates that when struck by a vehicle traveling forty miles per hour (mph; 64.4 km/h), a pedestrian has an 85 percent chance of death, and the fatality rate drops to 45 per- cent at thirty mph (48.2 km/h) and to 5 percent at twenty mph (32.2 km/h; UK Department of Transport 1997; Zegeer et al. 2002; ETSC 2005). Another study found higher rates of fatal- ities at even lower speeds (Tingvall and Haworth 1999). An analysis of vehicle impact speeds in pedestrian injuries in China found in cases where the vehicle was traveling less than twenty mph, there were no reported fatalities; collisions where the vehicle was traveling between twenty and twenty- five mph accounted for fewer than 5 percent of all fatalities (Zhao et al. 2010). A key finding in pedestrian safety research is that the single most consequential intervention in reducing pedestrian injury and fatality rates appears to be roadway treatments (Afukaar, Antwi, and Ofosu-Amaah 2003; Grundy et al. 2009; Mutabazi 2010; Methorst et al. 2010; Mohan and Tiwaria 1998; Hijar, Trostle, and Bronfman 2003; ETSC 1999). Vehicular speeds can be reduced by narrowing road- ways, using traffic-calming measures, and installing warning signs and frequent stop signs (Peden et al. 2004). These inter- ventions are most certainly within the realm of planners influence.

## *Conditions: Visibility*

Poor visibility is one of the greatest risk factors for pedestrians (Kwan and Mapstone 2006; Ulfarsson, Kim, and Booth 2010; Ackaah and Adonteng 2011). In the United States, 67 percent of all fatal vehicle–pedestrian collisions occur at night or under low-light conditions (Campbell et al. 2004; National Highway Traffic Safety Administration 2007; Zegeer et al. 2010). A sys- tematic analysis of the US Fatality Analysis Reporting System (FARS) data indicates that pedestrian fatalities increase as illu- mination decreases, holding other factors constant (Owens and Sivak 1996; Sullivan and Flannagan 2002; Griswold et al. 2011). Further analysis of FARS data reveals that twilight and the first hour of darkness typically result in the highest fre- quency of fatal collisions for pedestrian (Griswold et al. 2011). Because pedestrian volumes are often still high during twilight hours, pedestrian exposure (walking/crossing activity) during these time periods is the most deadly (Griswold et al. 2011).

Roadway lighting can improve the visibility of pedestrians, and proper design and timely maintenance of street lighting can, in turn, help improve the safety of the roadway system. Zhou and Hsu (2009) developed and installed a mobile lighting

measurement system in a test vehicle to collect luminance data along a corridor of US 19 in Pinellas County, Florida. Follow- ing the assessment, pedestrian crash data were collected for a three-year period. The results of the study demonstrated that nighttime pedestrian crashes were of higher frequency on poorly lit segments of roadway.

The risks of nighttime travel are demonstrably mitigated by the use of handheld lamps, flashing lights, and red and yellow retroreflective materials by pedestrians (Peden et al. 2004). Retroreflective materials are particularly effective when arranged in a ‘‘biomotion’’ configuration, which highlights the movement of the pedestrian (Peden et al. 2004). For nighttime visibility, handheld lamps, flashing lights, and red and yellow retroreflective materials have been found to increase pedestrian recognition (Peden et al. 2004).

# Considerations for Future Research

As research on pedestrian safety and the built environment con- tinues, we recommend the following for future research based on our current review of the literature. First, we suggest that researchers employ quasi-experimental research designs when- ever possible. Quasi-experimental research designs allow for improved understanding of causality between predictor vari- ables and pedestrian injuries. Cross-sectional or longitudinal designs were the most common research designs we observed (i.e., Jacobsen 2003; Tarko and Azam 2011; Afukaar, Antwi, and Ofosu-Amaah 2003). The insights drawn from studies using cross-sectional and longitudinal designs remain useful but can only offer correlational evidence between risk factors and pedestrian safety. Good examples of quasi-experimental research on pedestrian safety include LaScala, Johnson, and Gruenewald (2001) and Ewing, Chen, and Chen (2013). These studies move researchers and practitioners closer to under- standing the causality between risk factors, safety treatments, and pedestrian safety.

We also suggest that qualitative methodologies have much to offer the understanding of pedestrian safety and the built environment. Like quasi-experimental research, qualitative research is well suited to answer research questions that ask why? The majority of studies reviewed are purely quantitative (i.e., Clifton and Kreamer-Fults 2007; Petch and Henson 2000; Changcheng et al. 2010). We observed that some of the best studies we reviewed used mixed methods, employing both quantitative and qualitative research (Hijar, Vasquez-Vela, and Arreola-Risa 2003; LaScala, Johnson, and Gruenewald 2001). These studies moved beyond descriptions and summaries to answer why did a pedestrian injury occur? Employing mixed methodologies would further researcher and practitioner under- standing of pedestrian safety.

# Conclusion

This review has presented an overview of the evidence on risk factors for pedestrian road traffic injury in the built environ- ment by first examining research on pedestrians by type and

risk/safety factors, followed by research focused on different scales and aspects of the built environment. Three major factors that stand out are visibility, pedestrian–traffic interaction, and traffic speed. We conclude this article by reflecting on the question: ‘‘What do these findings on risk factors for pedes- trians in the built environment suggest planners need to do?’’ We are not saying that planners have not made an effort to address pedestrian safety in their work, but only pointing out that these findings remind this group of professionals about the importance of designing the built environment to reduce risks to pedestrians. Specifically, we see the following three

implications:

Risks factors in the built environment interact with each other to increase the probability of pedestrian fatalities and injuries occurring. Hence, the need for planners is to not only understand that these factors interact but also to consider them in risk assessments of the overall built environment during planning, implementation, and eva- luation of programs.

•

Address these risks during the design and implementation phases. Many pedestrian-friendly environmental features represent no added cost to implement during initial build- ing, meriting consideration, in all settings, whether high- or low-income countries. Because changes to the built environment are costly and difficult, thoughtful planning and design with pedestrian safety in mind becomes a cost-effective approach to reducing risks to pedes- trians. Planners can work toward reducing pedestrian risk by promoting strategies that encourage mixed land uses and accessibility. Specific measures to improve pedestrian safety such as reducing vehicle speed, reducing pedestrian exposure to vehicular traffic, and improving visibility between motor vehicles and pedestrians are available in literature (see, e.g., Zeeger et al. 2004; Retting, Ferguson, and McCartt 2003; Elvik et al. 2009).

•

Advocate for pedestrian safety. Planners can leverage their unique positions by urging public officials to develop and support policies that recognize the needs of pedestrians and by working with other local planners, designers, and developers to create pedestrian environ- ments that maximize pedestrian safety and well-being.

•

We have presented an overview of evidence from around the world, and it is up to the planners to utilize the evidence in their local and institutional settings.

Acknowledgments

This article is based on a literature review report that was prepared as a background resource for developing a pedestrian safety manual by the World Health Organization in 2013. The World Health Organiza- tion gratefully acknowledges the financial support received from Bloomberg Philanthropies and the US National Highway Traffic Safety Administration, which made possible the production of the pedestrian safety manual. We are also grateful for the contributions of M. Connors and J. Gulden.

Declaration of Conflicting Interests

The author(s) declared no potential conflicts of interest with respect to the research, authorship, and/or publication of this article.

Funding

The author(s) received no financial support for the research, author- ship, and/or publication of this article.

References

Ackaah, W., and D. O. Adonteng. 2011. ‘‘Analysis of Fatal Road Traf- fic Crashes in Ghana.’’ *International Journal of Injury Control and Safety Promotion* 18 (1): 21–27.

Afukaar, F. K., P. Antwi, and S. Ofosu-Amaah. 2003. ‘‘Pattern of Road Traffic Injuries in Ghana: Implications for Control.’’ *Injury Control and Safety Promotion* 10 (1–2): 69–76.

Agran, P. F., D. G. Winn, C. L. Anderson, and C. P. Del Valle. 1998. ‘‘Family, Social, and Cultural Factors in Pedestrian Injuries among Hispanic Children.’’ *Injury Prevention* 4:188–93.

Agran, P. F., D. G. Winn, C. L. Anderson, C. Tran, and C. P. Del Valle. 1996. ‘‘The Role of the Physical and Traffic Environment in Child Pedestrian Injuries.’’ *Pediatrics* 98 (6): 1096–103.

Al-Madani, H., and A. Al-Janahi. 2006. ‘‘Personal Exposure Risk Fac- tors in Pedestrian Accidents in Bahrain.’’ *Safety Science* 44 (4): 335–47.

Anderson, R. W. G., A. J. Mclean, M. J. B. Farmer, H. B. Lee, and C.

G. Brooks. 1997. ‘‘Vehicle Travel Speeds and the Incidence of Fatal Pedestrian Crashes.’’ *Accident Analysis & Prevention* 29 (5): 667–74.

Assailly, J. P. 1997. ‘‘Characterization and Prevention of Child Pedes- trian Accidents: An Overview.’’ *Journal of Applied Developmental Psychology* 18 (2): 257–62.

Avineri, E., D. Shinar, and Y. O. Susilo. 2012. ‘‘Pedestrians’ Beha- viour in Cross Walks: The Effects of Fear of Falling and Age.’’ *Accident Analysis & Prevention* 44 (1): 30–34.

Azetsop, J. 2010. ‘‘Social Justice Approach to Road Safety in Kenya: Addressing the Uneven Distribution of Road Traffic Injuries and Deaths across Population Groups.’’ *Public Health Ethics* 3 (2): 115–27.

Bartels, D., K. Bhalla, S. Shahraz, J. Abraham, R. Lozano, and C. J. L. Murray. 2010. ‘‘Incidence of Road Injuries in Mexico: Country Report.’’ *International Journal of Injury Control and Safety Pro- motion* 17 (3): 169–76.

Barton, B. K., and D. C. Schwebel. 2007. ‘‘The Influences of Demo- graphics and Individual Differences on Children’s Selection of Risky Pedestrian Routes.’’ *Journal of Pediatric Psychology* 32 (3): 343–53.

Berger, L. R., and D. Mohan. 1996. *Injury Control: A Global View*.

Oxford, UK: Oxford University Press.

Bhalla, K., M. Naghavi, S. Shahraz, D. Bartel, and C. J. L. Murray. 2009. ‘‘Building National Estimates of the Burden of Road Traffic Injuries in Developing Countries from All Available Data Sources: Iran.’’ *Injury Prevention* 15 (3): 150–56.

Bhatia, R., and M. Wier. 2011. ‘‘Safety in Numbers Re-examined: Can We Make Valid or Practical Inferences from Available Evidence?’’ *Accident Analysis & Prevention* 43 (1): 235–40.

Bishair, D., A. Quresh, P. James, and A. Ghaffar. 2006. ‘‘National Road Casualties and Economic Development.’’ *Health Economics* 15 (1): 65–81.

Boarnet, M., C. Anderson, K. Day, T. McMillan, and M. Alfonzo. 2005. ‘‘Evaluation of the California Safe Routes to School Legislation: Urban from Changes and Children’s Active Transportation to School.’’ *American Journal of Preventative Medicine* 28 (2): 134–40. Burden, D., and P. Lagerwey. 1999. *Road Diets: Fixing the Big Roads*. Washington, DC: Walkable Communities. Accessed November 7,

2012. [http://www.walkable.org/articles.html.](http://www.walkable.org/articles.html)

Campbell, B. J., C. V. Zegeer, H. H. Huang, and M. J. Cynecki. 2004. *A Review of Pedestrian Safety in the United States and Abroad*. Chapel Hill: University of North Carolina. Accessed December 2013. [ntl.](http://ntl.bts.gov/lib/24000/24700/24702/Ped_Synthesis_Report.pdf) [bts.gov/lib/24000/24700/24702/Ped\_Synthesis\_Report.pdf](http://ntl.bts.gov/lib/24000/24700/24702/Ped_Synthesis_Report.pdf).

Chakravarthy, B., C. L. Anderson, J. Ludlow, S. Lotfipour, and F. E. Vaca. 2010. ‘‘The Relationship of Pedestrian Injuries to Socioeco- nomic Characteristics in a Large Southern California County.’’ *Traffic Injury Prevention* 11 (5): 508–13.

Changcheng, L., G. Zhang, J. Zhang, and H. Zheng. 2010. ‘‘First Engi- neering Practice of Traffic Calming in Zhaitang Town in China.’’ Paper presented at the 2010 International Conference on Optoelec- tronics and Image Processing (ICOIP), Haikou, China. Published in ICOIP 1: 565–68.

Chen, Y., H. Meng, and Z. Wang. 2009. ‘‘Safety Improvement Prac- tice for Vulnerable Road Users in Beijing Intersections.’’ Paper presented at the 88th Annual Meeting of the Transportation Research Board, Washington, DC. Published in The TRB 88th Annual Meeting Compendium of Papers DVD.

Chow, D. H. K., M. L. Y. Kwok, A. C. K. Au-Yang, A. D. Holmes, J.

C. Y. Cheng, F. Y. D. Yao, and M. S. Wong. 2005. ‘‘The Effect of Backpack Load on the Gait of Normal Adolescent Girls.’’ *Ergo- nomics* 48 (6): 642–56.

Clark, J. 1985. *High Speeds and Volumes on Residential Streets: An Analysis of Physical Street Characteristics as Causes in Sacra- mento, California*. Compendium of Technical Papers. Washington, DC: Institute of Transportation Engineers.

Clayton, A., and M. Colgan. 2001. *Alcohol and Pedestrians—A Final Report to Road Safety Division*. Road Safety Research Report No.

20. London, UK: Department of the Environment, Transport and the Regions.

Clifton, K., and K. Kreamer-Fults. 2007. ‘‘An Examination of the Environmental Attributes Associated with Pedestrian-vehicular Crashes near Public Schools.’’ *Accident Analysis & Prevention* 39 (4): 708–15.

Collins, D. C. A., and R. A. Kearns. 2005. ‘‘Geographies of Inequality: Child Pedestrian Injury and Walking School Buses in Auckland, New Zealand.’’ *Social Sciences & Medicine* 60 (1): 61–69.

Constant, A., and E. Lagarde. 2010. ‘‘Protecting Vulnerable Road Users from Injury.’’ *PLoS Medicine* 7 (3): e1000228. doi:10. 1371/journal.pmed.1000228.

Cubbin, C. 2002. ‘‘Socioeconomic Inequalities in Injury: Critical Issues in Design and Analysis.’’ *Annual Review of Public Health* 23:349–75.

Dandona, R., G. A. Kumar, M. A. Ameer, G. M. Ahmed, and L. Dan- dona. 2008. ‘‘Incidence and Burden of Road Traffic Injuries in Urban India.’’ *Injury Prevention* 14 (6): 354–59.

Davies, D. G, Turner-Fairbank Highway Research Center, US Federal Highway Administration, University of North Carolina Highway Safety Research Center, and David Davies Associates. 1999. *Research, Development, and Implementation of Pedestrian Safety Facilities in the United Kingdom*. Mclean, VA: US Department of Transportation, US Federal Highway Administration, Turner- Fairbank Highway Research Center.

Delmelle, E. C., J. C. Thill, and H. H. Ha. 2012. ‘‘Spatial Epidemio- logic Analysis of Relative Collision Risk Factors among Urban Bicyclists and Pedestrians.’’ *Transportation* 39 (2): 433–48.

Demetriades, D., J. Murray, M. Martin, G. Velmahos, A. Salim, K. Alo, and P. Rhee. 2004. ‘‘Pedestrians Injured by Automobiles: Relationship of Age to Injury Type and Severity.’’ *Journal of the American Surgeons* 199 (3): 382–87.

Dumbaugh, E. 2005. ‘‘Safe Streets, Livable Streets: A Positive Approach to Urban Roadside Design.’’ Unpublished dissertation, Georgia Institute of Technology, Atlanta.

Dumbaugh, E., and W. Li. 2011. ‘‘Designing for the Safety of Pedes- trians, Cyclists, and Motorists in the Built Environment.’’ *Journal of the American Planning Association* 77 (1): 69–88.

Durak, D., R. Fedakar, N. Tu¨rkmen, S. Akgo¨z, and E. Badurog˘lu. 2008. ‘‘Road Traffic Collisions in Bursa, Turkey, during 2003, 2004 and 2005.’’ *Injury* 39 (5): 547–53.

Elvik, R., A. Hoye, T. Vaa, and M. Sorensen. 2009. *The Handbook of Road Safety Measures*. 2nd ed. Bingley, UK: Emerald Group Pub- lishing Limited.

ETSC (European Transport Safety Council). 1999. *Police Enforce- ment Strategies to Reduce Traffic Casualties*. Brussels, Belgium: ETSC. Accessed December 2013. [www.etsc.eu/documents/strate](http://www.etsc.eu/documents/strategies.pdf) [gies.pdf.](http://www.etsc.eu/documents/strategies.pdf)

ETSC (European Transport Safety Council). 2005. *Motor Vehicle Speed in the EU*. Brussels, Belgium: ETSC. Accessed February 7, 2012. [www.etsc.eu/documents/FS\_speed.pdf.](http://www.etsc.eu/documents/FS_speed.pdf)

Ewing, R., and R. Cervero. 2001. ‘‘Travel and the Built Environment: A Synthesis.’’ *Transportation Research Record: Journal of the Transportation Research Board* 1780:87–114.

Ewing, R., L. Chen, and C. Chen. 2013. ‘‘Quasi-experimental Study of Traffic Calming Measures in New York City.’’ *Transportation Research Record: Journal of the Transportation Research Board* 2364 (1): 29–35.

Ewing, R., and E. Dumbaugh. 2009. ‘‘The Built Environment and Traffic Safety: A Review of Empirical Evidence.’’ *Journal of Planning Literature* 23 (4): 347–67.

Ewing, R., R. Pendall, and D. Chen. 2002. *Measuring Sprawl and Its Impact*. Smart Growth America. Accessed December 15, 2011. [http://www.smartgrowthamerica.org/sprawlindex/Measur-](http://www.smartgrowthamerica.org/sprawlindex/MeasuringSprawl.pdf) [ingSprawl.pdf](http://www.smartgrowthamerica.org/sprawlindex/MeasuringSprawl.pdf).

Ewing, R., R. Schweiber, and C. V. Zegeer. 2003. ‘‘Urban Sprawl as a Risk Factor in Motor Vehicle Occupant and Pedestrian Fatalities.’’ *American Journal of Public Health* 93 (9): 1541–45.

Farouki, O. T., and W. J. Nixon. 1976. ‘‘The Effect of Width of Sub- urban Roads on the Mean Free Speed of Cars.’’ *Traffic Engineer- ing and Control* 17 (12): 518–19.

FHWA (Federal Highway Administration). 2001. *Geometric Design Practices for European Roads. Publication No. FHWA-PL-01-*

*026*. Washington, DC: US Department of Transportation.

Fitzpatrick, K., P. Carlson, M. Brewer, and M. Wooldridge. 2001. ‘‘Design Factors that Affect Driver Speed on Suburban Streets.’’ *Transportation Research Record* 1751:18–25.

Garder, P. E. 2004. ‘‘The Impact of Speed and Other Variables on Pedestrian Safety in Maine.’’ *Accident Analysis & Prevention* 36 (4): 533–42.

Gattis, J. L. 2000. ‘‘Urban Street Cross Section and Speed Issues.’’ Transportation Research E-circular. Transportation Research Board. Accessed December 2013. [ntl.bts.gov/lib/10000/10800/](http://ntl.bts.gov/lib/10000/10800/10868/Ec019_d3.pdf) [10868/Ec019\_d3.pdf.](http://ntl.bts.gov/lib/10000/10800/10868/Ec019_d3.pdf)

Gattis, J. L., and A. Watts. 1999. ‘‘Urban Street Speed Related to Width and Functional Class.’’ *Journal of Transportation Engineer- ing* 125 (3): 93–200.

Gawryszewski, V. P., and E. M. S. Rodrigues. 2006. ‘‘The Burden of Injury in Brazil.’’ *Sao Paulo Medicine Journal* 124 (4): 208–13.

Goren, S., M. Subasi, F. Gurkan, Y. Tirasci, and K. Acar. 2005. ‘‘Child Pedestrian Fatalities in Diyarbakir, Turkey.’’ *Saudi Medical Jour- nal* 26 (7): 1116–18.

Green, J., R. Ayrton, J. Woodall, J. Woodward, C. Newell, M. Cattan, and R. Cross. 2008. *Child–Parent Interaction in Relation to Road Safety Education: Part 2—Main Report: Road Safety Research Report 102*. Department of Transport. Accessed December 2013. [http://dera.ioe.ac.uk/1416/.](http://dera.ioe.ac.uk/1416/)

Griswold, J., B. Fishbain, S. Washington, and D. R. Ragland. 2011. ‘‘Visual Assessment of Pedestrian Crashes.’’ *Accident Analysis & Prevention* 43 (1): 301–06.

Grundy, C., R. Steinbach, P. Edwards, J. Green, B. Armstrong, and P. Wilkinson. 2009. ‘‘Effects of 20 mph Traffic Speed Zones on Road Injuries in London, 1986-2006: Controlled Interrupted Time Series Analysis.’’ *British Medical Journal* 339 (4469). Accessed Decem- ber 2013. [www.ncbi.nlm.nih.gov/pmc/articles/PMC2791801/pdf/](http://www.ncbi.nlm.nih.gov/pmc/articles/PMC2791801/pdf/bmj.b4469.pdf) [bmj.b4469.pdf.](http://www.ncbi.nlm.nih.gov/pmc/articles/PMC2791801/pdf/bmj.b4469.pdf)

Guth, D., D. Ashmead, R. Long, R. Wall, and P. Ponchillia. 2005. ‘‘Blind and Sighted Pedestrians’ Judgments of Gaps in Traffic at Roundabouts.’’ *Human Factors* 47 (2): 314–31.

Harwood, D. W. 1986. *Multilane Design Alternatives for Improving Suburban Highways*. NCHRP Report 282. Washington, DC: Transportation Research Board, National Research Council.

Harwood, D. W. 1990. *Effective Utilization of Street Width on Urban Arterials*. National Cooperative Highway Research Program Report 330. Washington, DC: National Research Council.

Harwood, D. W., D. J. Torbic, D. K. Gilmore, C. D. Bokenkoger, J. M. Dunn, C. V. Zegeer, S. Srinivasan, D. Carter, C. Raborn, C. Lyon, and B. Persaud. 2008. *Pedestrian Safety Prediction Methodology. Final Report for NCHRP Project 17-26*. Accessed December 2013. [onlinepubs.trb.org/onlinepubs/nchrp/nchrp\_w129p3.pdf.](http://onlinepubs.trb.org/onlinepubs/nchrp/nchrp_w129p3.pdf)

Hatfield, J., and S. Murphy. 2007. ‘‘The Effects of Mobile Phone Use on Pedestrian Crossing Behaviour and Signalised and Unsignalised Intersections.’’ *Accident Analysis & Prevention* 39 (1): 197–205.

Hauer, E. 1999. *Safety in Geometric Design Standards*. Accessed January 11, 2005. [www.researchgate.net/publication/228903642\_](http://www.researchgate.net/publication/228903642_Safety_in_geometric_design_standards/file/d912f5138f05bb6821.pdf) [Safety\_in\_geometric\_design\_standards/file/d912f5138f05bb6821.](http://www.researchgate.net/publication/228903642_Safety_in_geometric_design_standards/file/d912f5138f05bb6821.pdf) [pdf.](http://www.researchgate.net/publication/228903642_Safety_in_geometric_design_standards/file/d912f5138f05bb6821.pdf)

Heelan, K. A., B. M. Abbey, J. E. Donnelly, M. S. Mayo, and G. J. Welk. 2009. ‘‘Evaluation of a Walking School Bus for Promoting

Physical Activity in Youth.’’ *Journal of Physical Activity and Health* 6 (5): 560–67.

Heimbach, C. L., P. D. Cribbins, and M. S. Chang. 1983. ‘‘Some Par- tial Consequences of Reduced Traffic Lane Widths on Urban Arterials.’’ *Transportation Research Record* 923:69–72.

Hijar, M., J. Trostle, and M. Bronfman. 2003. ‘‘Pedestrian Injuries in Mexico: A Multi-method Approach.’’ *Social Science & Medicine* 57 (11): 2149–59.

Hijar, M., E. Vazquez-Vela, and C. Arreola-Risa. 2003. ‘‘Pedestrian Traffic Injuries in Mexico: A Country Update.’’ *Injury Control and Safety Promotion* 10 (1–2): 37–43.

Hilton, J. 2006. *Race and Ethnicity in Fatal Motor Vehicle Traffic Crashes 1999–2004*. Washington, DC: National Highway Traffic Safety Administration.

Holubowycz, O. T. 1995. ‘‘Age, Sex, and Blood Alcohol Concentra- tion of Killed and Injured Pedestrians.’’ *Accident Analysis & Prevention* 27 (3): 417–22.

Huang, H. G., J. R. Stewart, and C. V. Zegeer. 2002. ‘‘Evaluation of Lane Reduction ‘Road Diet’ Measure on Crashes and Injuries.’’ *Transportation Research Record* 1784:80–90.

Hummer, J. E., and C. F. Lewis. 2000. *Operational Capacity of Three- lane Cross-sections*. Raleigh: Center for Transportation Engineer- ing Studies, North Carolina State University.

Ibrahim, J. M., H. Day, J. Hirshon, and M. El-Seouhy. 2012. ‘‘Road Risk Perception and Pedestrian Injuries among Students and Ain Shams University, Cairo, Egypt.’’ *Injury & Violence Research* 4 (2): 65–72.

Ibrahim, S. E. B., and T. Sayed. 2011. ‘‘Developing Safety Perfor- mance Functions Incorporating Reliability-based Risk Measures.’’ *Accident Analysis & Prevention* 43 (6): 2153–59.

Jacobsen, P. L. 2003. ‘‘Safety in Numbers: More Walkers and Bicy- clists, Safer Walking and Bicycling.’’ *Injury Prevention* 9 (3): 205–9.

Job, R. F. S., J. Haynes, T. Prabhakar, S. H. V. Lee, and J. Quach. 1998. ‘‘Pedestrians at Traffic Light Controlled Intersections: Crossing Behaviour in the Elderly and Non-elderly.’’ In *Proceed- ings of the Conference on Pedestrian Safety*, edited by K. Smith, B.

G. Aitken, and R. H. Grzebieta, 3–11. Canberra: Australian Col- lege of Road Safety and Federal Office of Road Safety.

Kearns, R. A., D. C. A. Collins, and P. M. Neuwelt. 2003. ‘‘The Walk- ing School Bus: Extending Children’s Geographies?’’ *Area* 35 (3): 285–92.

Keigan, M., and R. Tunbridge. 2003. *The Incidence of Alcohol in Fatally Injured Adult Pedestrians*. TRL Report 579. Transporta- tion Research Laboratory. Accessed December 2013. [http://trid.](http://trid.trb.org/view.aspx?id=663709)

[trb.org/view.aspx?id](http://trid.trb.org/view.aspx?id=663709)¼[663709.](http://trid.trb.org/view.aspx?id=663709)

Kerr, J., D. Rosenberg, and L. Frank. 2012. ‘‘The Role of the Built

Environment in Healthy Aging: Community Design, Physical Activity, and Health among Older Adults.’’ *Journal of Planning Literature* 27 (1): 43–60.

Khayesi, M., H. Monheim, and J. M. Nebe. 2010. Negotiating ‘‘Streets for All’’ in Urban Transport Planning: The Case for Pedestrians, Cyclists and Street Vendors in Nairobi, Kenya.’’ *Antipode: A Rad- ical Journal of Geography* 42 (1): 103–26.

Kim, J., G. F. Ulfarssom, V. N. Shankar, and F. L. Mannering. 2010. ‘‘A Note on Modeling Pedestrian-injury Severity in Motor-vehicle

Crashes with the Mixed Logit Model.’’ *Accident Analysis & Pre- vention* 42 (6): 1751–58.

Knaap, K. K., and K. Giese. 2001. *Guidelines for the Conversion of Urban Four-lane Undivided Roadways to Three-lane Two-way Left-turn Facilities*. Ames, IA: Center for Transportation Research and Education and Iowa State University.

Kwan, I., and J. Mapstone. 2006. *Interventions for Increasing Pedes- trian and Cyclist Visibility for the Prevention of Death and Injuries*. Cochrane Database of Systematic Reviews 4. [http://info.onlineli-](http://info.onlinelibrary.wiley.com/userfiles/ccoch/file/Safety_on_the_road/CD003438.pdf) [brary.wiley.com/userfiles/ccoch/file/Safety\_on\_the\_road/CD003](http://info.onlinelibrary.wiley.com/userfiles/ccoch/file/Safety_on_the_road/CD003438.pdf) [438.pdf.](http://info.onlinelibrary.wiley.com/userfiles/ccoch/file/Safety_on_the_road/CD003438.pdf)

Kwan, I., and J. Mapstone. 2006. *Interventions for Increasing Pedes- trian and Cyclist Visibility for the Prevention of Death and Injuries*. The Cochrane Library. Accessed December 2013. [http://onlineli-](http://onlinelibrary.wiley.com/doi/10.1002/14651858.CD003438.pub2/abstract) [brary.wiley.com/doi/10.1002/14651858.CD003438.pub2/abstract.](http://onlinelibrary.wiley.com/doi/10.1002/14651858.CD003438.pub2/abstract) LaFiandra, M., R. C. Wagenaar, K. G. Holt, and J. P. Obusek. 2003. ‘‘How Do Load Carriage and Walking Speed Influence Trunk Coordination and Stride Parameters?’’ *Journal of Biomechanics*

36 (1): 87–95.

Lamm, R., B. Psarianos, and T. Mailender. 1999. *Highway Design and Traffic Safety Engineering Handbook*. New York: McGraw-Hill.

Langlois, J. A., P. M. Keyl, J. M. Guralnik, D. J. Foley, R. A. Maro- tolli, and R. B. Wallace. 1997. ‘‘Characteristics of Older Pedes- trians Who Have Difficulty Crossing the Street.’’ *American Journal of Public Health* 87 (3): 393–97.

LaScala, E., F. Johnson, and P. Gruenewald. 2001. ‘‘Neighborhood Characteristics of Alcohol-related Pedestrian Injury Collisions: A Geostatistical Analysis.’’ *Prevention Science* 2 (2): 123–34.

Lee, J., and F. Mannering. 1999. Analysis of Roadside Accident Frequency and Severity and Roadside Safety Management. *Final Research Report, Research Project T9903, Task 97: Analysis of Roadside Accident Severity & Roadside Safety Management*. Olympia, WA: Washington State Department of Transportation.

Litman, T., and S. Fitzroy. 2005. *Safe Travels: Evaluating Mobility Management Traffic Safety Impacts*. Victoria, Canada: Victoria Transport Policy Institute.

Lonero, L. P., K. M. Clinton, and D. Sleet. 2006. ‘‘Behavior Change Interventions in Road Safety.’’ In *Injury and Violence Prevention: Behavioral Science Theories, Methods and Applications*, edited by

A. C. Gielen, D. A. Sleet, and R. J. DiClemente, 213–33. San Fran- cisco, CA: Jossey-Bass.

Ma, W. J., S. P. Nie, H. F. Xu, Y. J. Xu, and Y. R. Zhang. 2010.

‘‘Socioeconomic Status and the Occurrence of Non-fatal Child Pedestrian Injury: Results from a Cross-sectional Survey.’’ *Safety Science* 48 (6): 823–28.

Marcin, J. P., M. Schembri, J. He, and P. S. Romano. 2003. ‘‘A Population-based Analysis of Socioeconomic Status and Insur- ance Status and Their Relationship with Pediatric Trauma Hospi- talization and Mortality Rates.’’ *American Journal of Public Health* 93 (3): 461–66.

Marshall, W. E., and N. W. Garrick. 2011. ‘‘Does Street Network Design Affect Traffic Safety?’’ *Accident Analysis & Prevention* 43 (3): 769–81.

McMahon, P. J., C. V. Zegeer, C. Duncan, R. L. Knoblauch, J. R. Stewart, and A. J. Khattak. 2002. *An Analysis of Factors*

*Contributing to ‘Walking along Roadway’ Crashes: Research Study and Guidelines for Sidewalks and Walkways. FHWA-RD- 01-101*. McLean, VA: Federal Highway Administration.

Mead, J., C. Zegeer, and M. Bushell. 2014. ‘‘Evaluation of Pedestrian- Related Roadway Measures: A Summary of Available Research.’’ P a BI Center. Chapel Hill, NC, UNC Highway safety Research Center, 115.

Mendoza, J. A., D. D. Levinger, and B. D. Johnston. 2009. ‘‘Pilot Eva- luation of a Walking School Bus Program in a Low-income Urban Community.’’ *BMC Public Health* 9:122. doi:10.1186/1471-2458- 9-122. Accessed December 2013. [http://www.biomedcentral.com/](http://www.biomedcentral.com/1471-2458/9/122) [1471-2458/9/122.](http://www.biomedcentral.com/1471-2458/9/122)

Methorst, R., H. Monterde i Bort, R. Risser, D. Sauter, M. Tight, and J. Walker. 2010. *Pedestrians’ Quality Needs. Final Report of the COST project 358*. PQN Project. Accessed December 2013. [http://www.walkeurope.org/final\_report/default.asp.](http://www.walkeurope.org/final_report/default.asp)

Milton, J., and F. Mannering. 1998. ‘‘The Relationship among High- way Geometrics, Traffic-related Elements and Motor-vehicle Accident Frequencies.’’ *Transportation* 25 (4): 395–413.

Moe, H. 2008. ‘‘Road Traffic Injuries among Patients Who Attended the Accident and Emergency Unit of the University of Malaya Medical Centre, Kuala Lumpur.’’ *Journal of the Malaya Medical Centre* 11 (1): 22–26.

Mohan, D., and G. Tiwaria. 1998. ‘‘Road Safety in Low-income Countries: Issues and Concerns Regarding Technology Transfer from High-income Countries.’’ In *Reflections on the Transfer of Traffic Safety Knowledge to Motorising Nations*, edited by Global Traffic Safety Trust, 27–56. Melbourne, Australia: ARRB Trans- port Research.

Mueller, B. A., F. P. Rivara, and A. B. Bergman. 1988. ‘‘Urban–Rural Location and the Risk of Dying in a Pedestrian–Vehicle Collision.’’ *The Journal of Trauma* 28 (1): 91–94.

Mutabazi, M. 2010. ‘‘Sight Obstruction at At-grade Pedestrian Cross- ings: A Review of the Understandings of the Meaning of Zigzag Lines.’’ *Safety Science* 48 (3): 283–87.

Nakitto, M. T., M. Mutto, A. Howard, and R. Lett. 2008. ‘‘Pedestrian Traffic Injuries among School Children in Kawempe, Uganda.’’ *African Health Sciences* 8 (3): 156–59.

Nasar, J., P. Hecht, and R. Wener. 2008. ‘‘Mobile Telephones, Dis- tracted Attention, and Pedestrian Safety.’’ *Accident Analysis & Prevention* 40 (1): 69–75.

Negrini, N. S., and R. Carabalona. 2002. ‘‘Backpacks On! Schoolchil- dren’s Perceptions of Load, Associations with Back Pain and Fac- tors Determining the Load.’’ *Spine* 27 (2): 187–95.

Neider, M. B., J. S. McCarley, J. A. Crowell, H. Kaczmarski, and A. F. Kramer. 2010. ‘‘Pedestrians, Vehicles, and Cell Phones.’’ *Accident Analysis & Prevention* 42 (2): 589–94.

NHTSA (National Highway Traffic Safety Administration). 2007. *Traffic Safety Facts 2006*. Washington, DC: National Highway Traffic Safety Administration. Accessed December 2013. [http://](http://mcs.nhtsa.gov/index.cfm?fuseaction=product.display&amp;product_ID=57)

[mcs.nhtsa.gov/index.cfm?fuseaction](http://mcs.nhtsa.gov/index.cfm?fuseaction=product.display&amp;product_ID=57)¼[product.display&product\_](http://mcs.nhtsa.gov/index.cfm?fuseaction=product.display&amp;product_ID=57) [ID](http://mcs.nhtsa.gov/index.cfm?fuseaction=product.display&amp;product_ID=57)¼[57](http://mcs.nhtsa.gov/index.cfm?fuseaction=product.display&amp;product_ID=57).

NJDOT (New Jersey Department of Transportation). 2007. *Pedestrian*

*Safety Management in New Jersey: A Strategic Assessment*. Tren- ton, NJ. Accessed August 13, 2013. [http://safety.fhwa.dot.gov/](http://safety.fhwa.dot.gov/ped_bike/ped_focus/expedaction/njersey/njersey.pdf) [ped\_bike/ped\_focus/expedaction/njersey/njersey.pdf.](http://safety.fhwa.dot.gov/ped_bike/ped_focus/expedaction/njersey/njersey.pdf)

Noland, R. B., and L. Oh. 2004. ‘‘The Effect of Infrastructure and Demographic Change on Traffic-related Fatalities and Crashes: A Case Study of Illinois County-level Data.’’ *Accident Analysis & Prevention* 36 (4): 525–32.

Odero, W., P. Garner, and A. Zwi. 1997. ‘‘Road Traffic Injuries in Devel- oping Countries: A Comprehensive Review of Epidemiological Studies.’’ *Tropical Medicine & International Health* 2 (5): 445–60.

Odero, W., M. Khayesi, and P. M. Heda. 2003. ‘‘Road Traffic Injuries in Kenya: Magnitude, Causes and Status of Intervention.’’ *Injury Control and Safety Promotion* 10 (1–2): 53–61.

OECD (Organisation for Economic Co-operation and Development).

1998. *Safety of Vulnerable Road Users*. Paris, France: OECD. Owens, D. A., and M. Sivak. 1996. ‘‘Differentiation of Visibility and

Alcohol as Contributors to Twilight Road Fatalities.’’ *Human Fac- tors* 38 (4): 680–89.

Peden, M. M. 2004. *World Report on Road Traffic Injury Prevention*.

Geneva, Switzerland: World Health Organization.

Peden, M. M., and A. Hyder. 2002. ‘‘Road Traffic Injuries are a Global Public Health Problem.’’ *British Medical Journal* 324:1153–59.

Peden, M. M., K. Oyegbite, J. Ozanne-Smith, A. Hyder, C. Branche,

A. F. Rahman, F. Rivara, and K. Bartolomeos, eds.. 2008. *World Report on Child Injury Prevention*. Geneva, Switzerland: World Health Organization and United Nations Children’s Fund.

Peden, M. M., R. Scurfield, D. Sleet, D. Modhan, A. Hyder, E. Jarawan, and C. Mathers, eds. 2004. *World Report on Road Traffic Injury Prevention*. Geneva, Switzerland: World Health Organization.

Petch, R. O., and R. R. Henson. 2000. ‘‘Child Road Safety in the Urban Environment.’’ *Journal of Transport Geography* 8 (3): 197–211.

Pitcairn, T. K., and T. Edlmann. 2000. ‘‘Individual Differences in Road Crossing Ability in Young Children and Adults.’’ *British Journal of Psychology* 91 (3): 391–410.

Pless, I. B., R. Verreault, and S. Tenina. 1989. ‘‘A Case-control Study of Pedestrian and Bicyclist Injuries in Childhood.’’ *American Jour- nal of Public Health* 79 (8): 995–98.

Ponnaluri, R., and F. Nagar. 2010. ‘‘Road Crash Risk among Vulnerable Population Groups in Andhra Pradesh, India.’’ Paper presented at the Transportation Research Board 89th Annual Meeting, Washington, DC. Porter, G. 2002. ‘‘Living in a Walking World: Rural Mobility and Social Equity Issues in Sub-Saharan Africa.’’ *World Development*

30 (2): 285–300.

Porter, G. 2008. ‘‘Transport Planning in Sub-Saharan Africa II: Put- ting Gender into Mobility and Transport Planning in Africa.’’ *Progress in Development Studies* 8 (3): 281–89.

Quaye, K., L. Leden, and E. Hauer, University of Toronto Department of Civil Engineering, and AAA Foundation for Traffic Safety. 1993. *Pedestrian Accidents and Left-turning Traffic as Signalized Inter- sections*. Washington, DC: AAA Foundation for Traffic Safety.

Retting, R., S. Ferguson, and A. McCartt. 2003. ‘‘A Review of Evidence-based Traffic Engineering Measures Designed to Reduce Pedestrian–Motor Vehicle Crashes.’’ *American Journal of Public Health* 93 (9): 1456–63.

Rivara, F., and M. Barber. 1985. ‘‘Demographic Analysis of Child- hood Pedestrian Injuries.’’ *Pediatrics* 76 (3): 375–81.

Roberts, I. 1995. ‘‘Adult Accompaniments and the Risk of Pedestrian Injury on the School–Home Journey.’’ *Injury Prevention* 1 (4): 242–44.

Roberts, I., R. Norton, R. Jackson, R. Dunn, and I. Hassal. 1995. ‘‘Effect of Environmental Factors on Risk of Injury of Child Pedes- trians by Motor Vehicles: A Case-control Study.’’ *British Medical Journal* 310 (6972): 91–94.

Rosenbloom, S., and M. Plessis-Fraissard. 2009. ‘‘Women’s Travel in Developed and Developing Countries: Two Versions of the Same Story?’’ Paper presented at the 4th International Conference on Women’s Issues in Transportation, Irvine, California. Published in *Transportation Research Board Conference Proceedings* 46: 63–77.

Roy, A. 2009. ‘‘Gender, Poverty, and Transportation in the Develop- ing World.’’ Paper presented at the 4th International Conference on Women’s Issues in Transportation, Irvine, California. Published in *Transportation Research Board Conference Proceedings* 46: 50–62.

RTMC (Road Traffic Management Corporation). 2009. *Easter 2009 Road Traffic Report*. Gauteng, South Africa. Accessed December 2013. [http://www.rtmc.co.za/index.php/reports/traffic-reports.](http://www.rtmc.co.za/index.php/reports/traffic-reports)

Salt Lake City. 2012. *Transportation—Crosswalk Flags*. Salt Lake City, UT. Accessed December 2013. [http://www.slcgov.com/](http://www.slcgov.com/transportation/transportation-crosswalk-flags) [transportation/transportation-crosswalk-flags.](http://www.slcgov.com/transportation/transportation-crosswalk-flags)

Sawalha, Z., and T. Sayed. 2001. ‘‘Evaluating Safety on Urban Arter- ial Roadways.’’ *Journal of Transportation Engineering* 127 (2): 151–58.

Schwebel, D. C., D. Stavrions, K. W. Byington, T. Davis, E. E. O’Neal, and D. de Jong. 2012. ‘‘Distraction and Pedestrian Safety: How Talking on the Phone, Texting, and Listening to Music Impact Crossing the Street.’’ *Accident Analysis & Prevention* 45 (2012): 266–71.

Seedat, M., S. MacKenzie, and D. Mohad. 2006. ‘‘The Phenomenol- ogy of Being a Female Pedestrian in an African and an Asian City: A Qualitative Investigation.’’ *Transportation Research Part F: Traffic Psychology and Behaviour* 9 (2): 139–53.

Shah, S. G. S., K. Khoumbati, and B. Soomro. 2007. ‘‘The Pattern of Deaths in Road Traffic Crashes in Sindh, Pakistan.’’ *International Journal of Injury Control and Safety Promotion* 14 (4): 231–39.

Sharples, P. M., A. Storey, A. Aynsley-Green, and J. A. Eyre. 1990. ‘‘Causes of Fatal Childhood Accidents Involving Head Injury in Northern Region, 1979–86.’’ *British Medical Journal* 301 (6762): 1193–97.

Siram, S. M., V. Sonaike, O. B. Bolorunduro, W. R. Greene, S. Z. Ger- ald, D. C. Chang, E. E. Cornwell, and T. A. Oyentunji. 2011. ‘‘Does the Pattern of Injury in Elderly Pedestrian Trauma Mirror That of the Younger Pedestrian?’’ *Journal of Surgical Research* 167 (1): 14–18.

Sleet, D. A., R. B. Naumann, and R. A. Rudd. 2011. ‘‘Injuries and the Built Environment.’’ In *Making Healthy Places: Designing and Building for Health, Well-being and Sustainability*, edited by A. L. Dannenberg, H. Frumkin, and R. J. Jackson, 77–90. Washington, DC: Island Press.

Small, T., and M. Sheedy. 2006. ‘‘Cost, Demographics and Injury Pro- file of Adult Pedestrian Trauma in Inner Sydney.’’ *ANZ Journal of Surgery* 76 (1–2): 43–47.

Stavrinos, D., K. Byington, and D. Schwebel. 2009. ‘‘Effect of Cell Phone Distraction on Pediatric Pedestrian Injury Risk.’’ *Pediatrics* 123 (2): 179–85.

Sullivan, J. M., and M. J. Flannagan. 2002. ‘‘The Role of Ambient Light Level in Fatal Crashes: Interferences from Daylight Savings Time Transitions.’’ *Accident Analysis & Prevention* 34 (4): 487–89.

Swift, P., D. Painter, and M. Goldstein. 2006. ‘‘Residential Street Typology and Injury Accident Frequency.’’ Accessed December 2013. [massengale.typepad.com/venustas/files/SwiftSafetyStudy.](http://massengale.typepad.com/venustas/files/SwiftSafetyStudy.pdf) [pdf](http://massengale.typepad.com/venustas/files/SwiftSafetyStudy.pdf).

SWOV (Institute for Road Safety Research). 1993. *Towards a Sustain- able Safe Traffic System in the Netherlands*. Leidschendam, the Netherlands: Institute for Road Safety Research.

Tarko, A., and S. Azam. 2011. ‘‘Pedestrian Injury Analysis with Con- sideration of the Selectivity Bias in Linked Police–Hospital Data.’’ *Accident Analysis & Prevention* 43 (5): 1689–95.

Tingvall, C., and N. Haworth. 1999. ‘‘Vision Zero: An Ethical Approach to Safety and Mobility.’’ Paper presented at the 6th Insti- tute of Transport Engineers International Conference on Road Safety and Traffic Enforcement: Beyond 2000, Melbourne, Aus- tralia. Accessed October 30, 2003. [www.general.monash.edu.au/](http://www.general.monash.edu.au/MUARC/viszero.htm) [MUARC/viszero.htm.](http://www.general.monash.edu.au/MUARC/viszero.htm)

Tom, A., and M. A. Granie´. 2011. ‘‘Gender Differences in Pedes- trian Rule Compliance and Visual Search at Signalized and Unsignalized Crossroads.’’ *Accident Analysis & Prevention* 43 (5): 1794–801.

Toroyan, T. 2009. *Global Status Report on Road Safety: Time for Action*. Geneva, Switzerland: World Health Organization.

UK Department of Transportation. 1997. *Killing Speed and Saving Lives*. London, UK: UK Department of Transport.

Ulfarsson, G. F., S. Kim, and K. M. Booth. 2010. ‘‘Analyzing Fault in Pedestrian–Motor Vehicle Crashes in North Carolina.’’ *Accident Analysis & Prevention* 42 (6): 1805–13.

United Nations, Department of Economic and Social Affairs, Popula- tion Division. 2013. *World Population Ageing 2013*. New York: United Nations.

Untermann, R. K. 1990. ‘‘Street Design—Reassessing the Function, Safety, and Comfort of Streets for Pedestrians.’’ Paper presented at the 11th International Pedestrian Conference—The Road Less Traveled: Getting There by Other Means, Boulder, CO.

Vanderschuren, M., and R. Jobanputra. 2009. ‘‘Traffic Calming Mea- sures: Review and Analysis.’’ Working Paper 16-02, Cape Town, African Centre of Excellence for Studies in Public and Non- motorized Transport.

Vitaliano, D. F., and J. Held. 1991. ‘‘Road Accident External Effect: An Empirical Assessment.’’ *Applied Econometrics* 23 (2): 373–78. Vyrostek, S. B., J. L. Annest, and G. W. Ryan. 2004. *Surveillance for Fatal and Nonfatal Injuries—United States, 2001*. Atlanta, GA: Centers for Disease Control and Prevention. Accessed March 4, 2008. [http://www.cdc.gov/mmwR/preview/mmwrhtml/ss5307a1.](http://www.cdc.gov/mmwR/preview/mmwrhtml/ss5307a1.htm)

[htm.](http://www.cdc.gov/mmwR/preview/mmwrhtml/ss5307a1.htm)

Walker, E. J., S. N. Lanthier, E. F. Risko, and A. Kingstone. 2012. ‘‘The Effects of Personal Music Devices on Pedestrian Beha- viour.’’ *Safety Science* 50 (1): 123–28.

Wang, Y. T., D. D. Pascoe, and W. Weimar. 2001. ‘‘Evaluation of Book Backpack Load during Walking.’’ *Ergonomics* 44 (9): 858–69.

Wanvik, P. 2009. ‘‘Effects of Road Lighting: An Analysis Based on Dutch Accident Statistics 1987–2006.’’ *Accident Analysis & Pre- vention* 41 (1): 123–28.

Whitelegg, J. 1993. *Transport for a Sustainable Future: The Case for Europe*. London, UK: Belhaven.

Whitelegg, J. 2012. *Quality of Life and Public Management: Redefin- ing Development in the Local Environment*. Oxon, UK: Routledge. Wilkinson, R., and M. Marmot, eds. 2003. *Social Determinants of Health: The Solid Facts*. 2nd ed. Copenhagen, Denmark: World

Health Organization.

Woonerfgoed Network. 2014. Accessed November 2014. [http://www.](http://www.woonerfgoed.nl/int/Welcome.html) [woonerfgoed.nl/int/Welcome.html.](http://www.woonerfgoed.nl/int/Welcome.html)

World Health Organization. 2002. *The World Health Report 2002: Reducing Risks, Promoting Healthy Life*. Geneva, Switzerland: World Health Organization.

World Health Organization. 2009. *Global Status Report on Road Safety: Time for Action*. World Health Organization. Accessed November 2014. [http://www.who.int/violence\_injury\_prevention/](http://www.who.int/violence_injury_prevention/road_safety_status/2009/en/) [road\_safety\_status/2009/en/.](http://www.who.int/violence_injury_prevention/road_safety_status/2009/en/)

World Health Organization. 2013a. *Global Status Report on Road Safety 2013: Supporting a Decade of Action*. Geneva, Switzerland: World Health Organization.

World Health Organization. 2013b. *Pedestrian Safety: A Road Safety Manual for Decision-makers and Practitioners*. World Health Organization. Accessed August 25, 2013. [http://www.who.int/](http://www.who.int/roadsafety/projects/manuals/pedestrian/en/) [roadsafety/projects/manuals/pedestrian/en/.](http://www.who.int/roadsafety/projects/manuals/pedestrian/en/)

Xiang, H., M. Zhu, S. A. Sinclair, L. Stallones, J. R. Wilkins III, and

G. A. Smith. 2006. ‘‘Risk of Vehicle–Pedestrian and Vehicle– Bicyclist Collisions among Children with Disabilities.’’ *Accident Analysis & Prevention* 38 (6): 1064–70.

Xie, Y., Y. Ying, G. Xu, Y. Hu, and P. He. 2002. ‘‘Analysis on the Mortality Level of Injury among Floating Population in Urban Dis- trict of Ningbo from 1997 to 2000.’’ *Chinese Journal of Disease Control and Prevention* 6 (2): 185–86.

Zahabi, S. A. H., J. Strauss, K. Manaugh, and L. F. Miranda-Moreno. 2011. ‘‘Estimated Potential Effect of Speed Limits, Built Envi- ronment, and Other Factors on Severity of Pedestrian and Cyclist Injuries in Crashes.’’ *Transportation Research Record* 2247: 81–90.

Zegeer, C. V., and M. Bushell. 2012. ‘‘Pedestrian Crash Trends and Potential Countermeasures from Around the World.’’ *Accident Analysis & Prevention* 44 (1): 3–11.

Zegeer, C., D. Nabors, D. Gelinne, N. Lefler, and M. Bushell. 2010. ‘‘Pedestrian Safety Strategic Plan: Recommendations for Research and Product Development’’ (No. FHWA-10-035).

Zegeer, C. V., C. Seiderman, P. Lagerwey, M. Cynecki, M. Ronkin, and R. Schneider. 2002. *Pedestrian Facilities Users Guide— Providing Safety and Mobility*. Chapel Hill, NC: Highway Safety Research Center.

Zeeger, C. V., J. Stutts, H. Huang, M. J. Cynecki, H. Van Houten, B. Alberson, R. Pferer, T. R. Neuman, K. L. Slackand, and K. K. Hardy. 2004. *Guidance for Implementation of AASHTO Strategic Highway Safety Plan: Volume 10: A Guide for Reducing Collisions Involving Pedestrians*. Washington, DC: Transportation Research Board.

Zhao, H., Z. Yin, R. Chen, H. Chen, C. Song, G. Yang, and Z. Wang. 2010. ‘‘Investigation of 184 Passenger Car–Pedestrian Accidents.’’ *International Journal of Crashworthiness* 15 (3): 313–20.

Zhou, H., and P. Hsu. 2009. ‘‘Effects of Roadway Lighting Level on the Pedestrian Safety.’’ Paper presentation at the 9th International

Conference of Chinese Transportation Professionals, Harbin, China. Accessed December 2013. [http://ascelibrary.org/doi/abs/](http://ascelibrary.org/doi/abs/10.1061/41064%28358%294) [10.1061/41064](http://ascelibrary.org/doi/abs/10.1061/41064%28358%294)%[28358](http://ascelibrary.org/doi/abs/10.1061/41064%28358%294)%[294.](http://ascelibrary.org/doi/abs/10.1061/41064%28358%294)

Author Biographies

Philip Stoker is a graduate of the department of City and Metropoli- tan Planning at the University of Utah. He has a master’s degree in

Resource and Environmental Management and a Bachelor of Science in Environmental Management. He has conducted environmental and social science research internationally, including work with the World Health Organization, Parks Canada, the National Park Service, and the Vancouver 2010 Olympic Games.

Andrea Garfinkel-Castro is currently completing her PhD in Metro- politan Planning, Policy, and Design at the University of Utah. Her dissertation research examines sociocultural gaps in planning educa- tion and practice and how planners, faculty, and communities navigate the need to accommodate growing urban diversity.

Meleckidzedeck Khayesi was born in Vihiga District, Kenya. He is a teacher by profession with a bachelor of education degree (1988), a master of arts degree in geography (1992), and a doctor of philosophy degree in transport geography (1999). He facilitates development, implementation, and evaluation of road safety programs in countries and road safety capacity development.

Wilson Odero is a public health physician and currently dean, School of Medicine at Maseno University, Kenya. After obtaining his MD, he completed masters and PhD in Epidemiology and Public Health at the

London School of Hygiene & Tropical Medicine. He later undertook postdoctoral fellowship in medical informatics at Indiana University. He has published widely on various subjects of public health importance, with a focus on road traffic injuries and violence in developing countries.

Martin N. Mwangi is a public health nutritionist and epidemiologist and currently a researcher, School of Public Health and Community Development, at Maseno University, Kenya. He obtained both his MSc

in Public Health Nutrition and Epidemiology and PhD in Human Nutri- tion from Wageningen University, the Netherlands. He was granted a postdoctoral fellowship at Wageningen University and specialized in nutrition, health, and epidemiological research in East and West Africa.

Margie Peden is currently the coordinator of the Unintentional Inju- ries Prevention unit (UIP) within the Department for Management of Noncommunicable Diseases, Disability, Violence, and Injury Preven- tion at the World Health Organization in Geneva, Switzerland. She

coordinates work in the areas of unintentional injury prevention (including road safety, drowning, and burns prevention), injury sur- veillance/surveys, and alcohol and drug-related injuries.

Reid Ewing, PhD, is a professor of City and Metropolitan Planning at the University of Utah, associate editor of the *Journal of the American Planning Association*, editorial board member of the *Journal of Plan-*

*ning Education and Research*, and columnist for *Planning* magazine, writing the bimonthly column Research You Can Use. He has exten- sively studied that relationship between land use patterns, street design, and traffic safety, coauthoring the earlier *Journal of Planning Literature* article ‘‘The Built Environment and Traffic Safety: A Review of Empirical Evidence.’’